RC522 RFID-Device

<https://github.com/pkourany/MFRC522_RFID_Library>

Pinouts for the RC522 to Arduino Uno

MOSI: Pin 11

MISO: Pin 12

SCK: Pin13

SS: Pin 10

RST: Pin 9

I2C LC-Display

<https://github.com/fdebrabander/Arduino-LiquidCrystal-I2C-library>

PCF8574

the Adress I2C 0x20 for init the LC-Display